PACK 54 FISHKILL
PINEWOOD DERBY RULES – Clydesdale Race

The cars will be checked and inspected at registration for the following:

**1) There is NO minimum or Maximum weight.**

2) The width shall no exceed 2 ¾ inches.

3) The length shall not exceed 7 inches.

4) It is recommended that the car be no taller than 6 inches in height from wheel base in order to clear the timing gate at the finish line. If the car would hit the gate at the end of the track it will not be allowed to race.

**5) Axles, wheels and body CAN be modified and non BSA wheels may be used.**

6) Gravity will be the only force to propel the car. No motors, wind up spring, or propellents may be used to further enhance the travel of your car.

7) Any details added must be within the length, height and width limits.

8) We recommend that no items be attached to the bottom of the car. This will not make the car illegal, however, due to very little clearance between the car bottom and the track this will likely impede the cars ability to race.

9) ONLY DRY LUBRICANTS ARE ALLOWED so as to not damage the track

10) Cars should not be designed in such a way that they would present a danger to damage the track and/or other cars or interfere with any other car’s ability to run down adjacent tracks.

11) Keep in mind that once you check your car in for your race you will not be allowed to handle it again until all races within your division are finished. If your car is damaged during the race in such a way that would impair its ability to continue, ie a wheel falls off; ***at the judge’s discretion*** you may be given the opportunity to make a quick repair (maximum 2 minutes) or one may be made by a member of the “pit crew” to restore the car to running condition. Any non-essential pieces that may separate from the car will be set aside and the car will complete its races as is.

12)  The decision of the Official Car Inspectors and Judges is Final.